List all options for specifying board information.

class pyulwin.enums.BoardInfo

Member | Value
ACCOUPLED | 218
ACTUALDAQSCANRATE | 275
ADAIMODE | 373
ADBRIDGETYPE | 290
ADCAVGCOUNT | 302
ADCCALIBRATE | 267
ADCCALSTEPS | 268
ADCFG | 117
ADCHANAIMODE | 249
ADCHANMODE | 313
ADCHANTYPE | 355
ADCHANTYPES | 325
ADCPACEROUT | 252
ADCSETTLETIME | 270
ADDATARATE | 362
ADDIFFRANGE | 315
ADEXCITATION | 289
ADFIFOSIZE | 220
ADHASPACER | 324
ADINPUTMODE | 118
ADLOADCALCOEFS | 294
ADMAXBURSTRATE | 322
ADMAXBURSTTHROUGHPUT | 323
ADMAXDIFFQUEUELENGTH | 328
ADMAXRATE | 320
ADMAXSEQUEUELENGTH | 327
ADMAXTHROUGHPUT | 321
ADNUMCHANMODES | 312
ADNUMDIFFRANGES | 314
ADNUMSERANGES | 316
ADNUMTRIGTYPES | 318
ADPOLARITY | 112
ADQUEUELIMITS | 330
ADQUEUETYPES | 329
ADRES | 291
ADSCANOPTIONS | 326
ADSERANGE | 317
ADSOURCE | 221
ADTIMINGMODE | 285
ADTRIGCOUNT | 219
ADTRIGSRC | 209
ADTRIGTYPE | 319
ADXFERMODE | 306
AIWAVETYPE | 202
ATRIGCALIBRATE | 288
ATRIGRANGE | 300
BASEADR | 0
BNCSRC | 210
BNCTHRESHOLD | 211
BOARDTEMP | 226
BOARDTYPE | 1
BURSTMODE | 212
BUSNUM | 257
BUTTONSTATE | 297
CALDACVREF | 281
CALFACTOR1 | 146
CALFACTOR2 | 147
CALOUTPUT | 222
CALTABLETYPE | 254
CALTIMEOUT | 293
CHANBRIDGETYPE | 354
CHANBWMODE | 279
CHANCFG | 149
CHANRTDTYPE | 356
CHANTCTYPE | 347
CIDEVNUM | 12
CINUMDEVS | 11
CLOCK | 5
CLOCKTIME | 296
COMADDR2 | 151
CONNECTED | 342
CTLRNUM | 206
CTR0SRC | 104
CTR10SRC | 161
CTR11SRC | 162
CTR12SRC | 163
CTR13SRC | 164
CTR14SRC | 165
CTR1SRC | 105
CTR2SRC | 106
CTR3SRC | 130
CTR4SRC | 131
CTR5SRC | 132
CTR6SRC | 157
CTR7SRC | 158
CTR8SRC | 159
CTR9SRC | 160
CTRINTSRC | 133
CTRLINKING | 134
CTRLLINES | 154
CTRSCANOPTIONS | 369
CTRTRIGCOUNT | 307
CTSRTS1 | 152
CTSRTS2 | 153
CURRENTGATEWAYIP | 243
CURRENTIP | 232
CURRENTPORT | 234
CURRENTSUBNET | 245
DAC0VREF | 108
DAC1VREF | 109
DACCALIBRATE | 299
DACCALVOLT | 282
DACDEVRANGE | 335
DACDISABLERESTORE | 375
DACFIFOSIZE | 333
DACFORCESENSE | 250
DACHASPACER | 331
DACINSTALLED | 116
DACLOADCALCOEFS | 295
DACNUMRANGES | 334
DACNUMTRIGTYPES | 336
DACPACEROUT | 253
DACPOLARITY | 119
DACRANGE | 114
DACRES | 292
DACRESTORE | 217
DACSAMPLEHOLD | 100
DACSCANOPTIONS | 332
DACSTARTUP | 217
DACTRIG | 148
DACTRIGCOUNT | 284
DACTRIGTYPE | 337
DACUPDATE | 115
DACUPDATECMD | 216
DACUPDATEMODE | 215
DACXFERPRIMECOUNT | 277
DAQAMISUPPORTED | 338
DAQICHANTYPE | 377
DAQINUMCHANTYPES | 376
DAQISCANOPTIONS | 370
DAQITRIGCOUNT | 308
DAQOCHANTYPE | 379
DAQONUMCHANTYPES | 378
DAQOSCANOPTIONS | 371
DEFAULTGATEWAYIP | 244
DEFAULTIP | 231
DEFAULTSUBNET | 246
DETECTOPENTC | 361
DEVCLASS | 372
DEVINST | 303
DEVIPADDR | 374
DEVMACADDR | 364
DEVNOTES | 263
DEVSERIALNUM | 363
DEVUNIQUEID | 357
DEVVERSION | 359
DHCPENABLED | 233
DIALARMMASK | 230
DIDEBOUNCESTATE | 255
DIDEBOUNCETIME | 256
DIDEVNUM | 10
DIFILTERTIME | 304
DINUMDEVS | 9
DIOENABLE | 101
DISCANOPTIONS | 367
DISCONNECT | 340
DISOFILTER | 122
DISTATERETENTION | 305
DITHERON | 213
DITRIGCOUNT | 343
DMACHAN | 3
DOSCANOPTIONS | 368
DOTRIGCOUNT | 344
DTBOARD | 17
EXCITATION | 353
EXTCLKTYPE | 227
EXTINPACEREDGE | 348
EXTOUTPACEREDGE | 349
EXTPOWERSTATE | 278
FACTORYID | 272
FWVERSION | 170
HASEXTINFO | 309
HIDELOGINDLG | 274
HTTPPORT | 273
INDEXCFG | 200
INITIALIZED | 4
INPUTPACEROUT | 350
INT32PRIORITY | 124
INT32SRC | 123
INTEDGE | 265
INTERFACEPATH | 298
INTLEVEL | 2
INTP1LEVEL | 156
INTP2LEVEL | 110
IODEVTYPE | 311
IRQCONNECT | 204
LEDPATTERN | 301
MEMCOUNT | 126
MEMSIZE | 125
MFGSERIALNUM | 224
NETBIOSNAME | 366
NETCONNECTCODE | 341
NETIOTIMEOUT | 247
NETMINPORT | 248
NODEID | 262
NOITEM | 99
NUMADCHANS | 7
NUMDACHANS | 13
NUMEXPS | 18
NUMIODEVS | 310
NUMIOPORTS | 15
NUMTEMPCHANS | 208
OPENRELAYLEVEL | 229
OUTPUTPACEROUT | 351
OWNERIP | 240
OWNERNAME | 239
PACERCTR0SRC | 107
PANID | 258
PARENTBOARD | 16
PATTERNTRIGPORT | 345
PCIREVID | 225
PHACFG | 180
PHBCFG | 190
POWERLEVEL | 260
PPIODIO | 129
PRNDELAY | 128
PRNPORT | 127
PROGRAMDEV | 264
PROTOCOL | 150
PWRJMPR | 207
PWRUPSTATE | 203
RANGE | 6
RELAYLOGIC | 228
RFCHANENERGY | 266
RFCHANNEL | 259
RSS | 261
RTDCHANTYPE | 286
SBX0ADDRESS | 136
SBX0BOARDNUM | 135
SBX0DMACHAN | 137
SBX0INTLEVEL0 | 138
SBX0INTLEVEL1 | 139
SBX1ADDRESS | 141
SBX1BOARDNUM | 140
SBX1DMACHAN | 142
SBX1INTLEVEL0 | 143
SBX1INTLEVEL1 | 144
SBXBUSWIDTH | 145
SERIALNUM | 214
SLOTNUM | 201
SRCADPACER | 223
SYNCMODE | 251
TBASERES | 241
TCCHANRANGE | 168
TCCHANTYPE | 169
TCCJCSTATE | 167
TCGLOBALAVG | 166
TEMPAVG | 352
TEMPCALIBRATE | 242
TEMPCALSTEPS | 269
TEMPCHANGAIN | 238
TEMPCONNECTIONTYPE | 236
TEMPEXCITATION | 237
TEMPMODE | 120
TEMPREJFREQ | 121
TEMPSCALE | 280
TEMPSENSORTYPE | 235
TERMCOUNTSTATBIT | 360
TERMINALCOUNTSTATUSENABLE | 287
TRIGEDGE | 113
TRIGPOLARITY | 205
USBQUERY | 276
USERADCSETTLETIME | 283
USERDEVID | 358
USERDEVIDNUM | 365
USESEXPS | 8
WAITSTATE | 14
WAITSTATEP1 | 155
WAITSTATEP2 | 111
WEBSERVERENABLE | 271