## MEGA-FIFO

The MEGA-FIFO supports the following UL and UL for .NET features.

Memory I/O

Only used in combination with a board which has DT-Connect.

Functions

UL: cbMemSetDTMode(), cbMemReset(), cbMemRead(), cbMemWrite(), cbMemReadPretrig()

UL for .NET: MemSetDTMode(), MemReset(), MemRead(), MemWrite(), MemReadPretrig()

Some of these functions are integrated into the cbAInScan() function and AInScan() method. For example, if you use MEGA-FIFO with an A/D board and select the EXTMEMORY option, you would not have to call the cbMemSetDTMode() and cbMemWrite()functions or the MemSetDTMode() and MemWrite() methods.

EXTMEMORY option

Continuous mode cannot be used with the EXTMEMORY/ExtMemory option.