# BoardConfig.GetBaseAdr() method

Gets the base address used by the Universal Library to communicate with a board. This is recommended for use only with ISA bus boards.

Member of the cBoardConfig class. Accessible from the MccBoard.BoardConfig property.

## Function Prototype

VB .NET

Public Function GetBaseAdr(ByVal devNum As Integer, ByRef configVal As Integer) As MccDaq.ErrorInfo

C# .NET

public MccDaq.ErrorInfo GetBaseAdr(int devNum, out int configVal)

## Parameters

devNum

Number of the base address to return (PCI boards may have several address ranges).

configVal

The board's base address.

## Returns

- An ErrorInfo object that indicates the status of the operation.