# BoardConfig.SetAdTimingMode()

Sets the ADC timing mode.

Member of the cBoardConfig class. Accessible from the MccBoard.BoardConfig property.

## Function Prototype

VB .NET

Public Function SetAdTimingMode(ByRef configVal As Integer) As MccDaq.ErrorInfo

C# .NET

public MccDaq.ErrorInfo SetAdTimingMode(int configVal)

## Parameters

configVal

The ADC timing mode. Valid values are 1 (High Speed), 8 (60 Hz rejection), 9 (50 Hz rejection), and 15 (High resolution).

## Returns

- An ErrorInfo object that indicates the status of the operation.