Defines the set of ranges within the UL for A/D and D/A operations.

public enum MccDaq.Range

Constant name | Range | Value
Bip60Volts | ±60 volts | 20
Bip20Volts | ±20 volts | 15
Bip15Volts | ±15 volts | 21
Bip10Volts | ±10 volts | 1
Bip5Volts | ±5 volts | 0
Bip4Volts | ±4 volts | 16
Bip2Pt5Volts | ±2.5 volts | 2
Bip2Volts | ±2 volts | 14
Bip1Pt67Volts | ±1.67 volts | 11
Bip1Pt25Volts | ±1.25 volts | 3
Bip1Volts | ±1 volts | 4
BipPt625Volts | ±0.625 volts | 5
BipPt5Volts | ±0.5 volts | 6
BipPt312Volts | ±0.3125 volts | 17
BipPt25Volts | ±0.25 volts | 12
BipPt2Volts | ±0.2 volts | 13
BipPt156Volts | ±0.15625 volts | 18
BipPt125Volts | ±0.125 volts | 22
BipPt1Volts | ±0.1 volts | 7
BipPt078Volts | ±0.078125 volts | 19
BipPt05Volts | ±0.05 volts | 8
BipPt01Volts | ±0.01 volts | 9
BipPt005Volts | ±0.005 volts | 10
Uni10Volts | 0 - 10 volts | 100
Uni5Volts | 0 - 5 volts | 101
Uni4Volts | 0 - 4 volts | 114
Uni2Pt5Volts | 0 - 2.5 volts | 102
Uni2Volts | 0 - 2 volts | 103
Uni1Pt67Volts | 0 - 1.67 volts | 109
Uni1Pt25Volts | 0 - 1.25 volts | 104
Uni1Volts | 0 - 1 volts | 105
UniPt5Volts | 0 - 0.5 volts | 110
UniPt25Volts | 0 - 0.25 volts | 111
UniPt2Volts | 0 - 0.2 volts | 112
UniPt1Volts | 0 - 0.1 volts | 106
UniPt01Volts | 0 - 0.01 volts | 107
UniPt02Volts | 0 - 0.02 volts | 108
UniPt05Volts | 0 - 0.05 volts | 113
Ma4To20 | 4 - 20 mA | 200
Ma2To10 | 2 - 10 mA | 201
Ma1To5 | 1 - 5 mA | 202
MaPt5To2pt5 | 0.5 - 2.5 mA | 203
Ma0To20 | 0 - 20 mA | 204
BipPt025Amps | ±0.025 amps | 205
Not Used |  | –1