# BoardConfig.SetBaseAdr()

Sets the base address used by the Universal Library to communicate with a board. This is recommended for use only with ISA bus boards.

Member of the cBoardConfig class. Accessible from the MccBoard.BoardConfig property.

## Function Prototype

VB .NET

Public Function SetBaseAdr(ByVal devNum As Integer, ByVal configVal As Integer) As MccDaq.ErrorInfo

C# .NET

public MccDaq.ErrorInfo SetBaseAdr(int deveNum, int configVal)

## Parameters

devNum

Number of the base address to configure (should always be 0 – can't configure PCI base addresses).

configVal

Sets the base address of the board.

## Returns

- An ErrorInfo object that indicates the status of the operation.