# CIO-DAS08/JR Series

The CIO-DAS08/JR Series includes the following hardware:

- CIO-DAS08/JR
- CIO-DAS08/JR-AO
- CIO-DAS08JR/16
- CIO-DAS08/JR/16-AO

The CIO-DAS08/JR Series support the following UL and UL for .NET features.

## Analog Input

Functions

UL: cbAIn(), cbAInScan(), cbATrig(), cbFileAInScan()

UL for .NET: AIn(), AInScan(), ATrig(), FileAInScan()

Options

CONVERTDATA

HighChan

0 to 7

Rate

Ignored

Range

These boards do not have programmable gain, so the Range arguments for analog input functions are ignored.

## Analog Output

Valid if the optional D/A converters are installed on the board.

Functions

UL: cbAOut(), cbVOut(), cbAOutScan()

UL for .NET: AOut(), VOut(), AOutScan()

Options

SIMULTANEOUS

HighChan

1 max

Rate

Ignored

Count

2 max

Range

Ignored - not programmable; fixed at BIP5VOLTS (±5 volts)

DataValue

0 to 4,095

For the CIO-DAS08/JR/16-AO, the following argument values are also valid:

0 to 65,535 (Refer to 16-bit values using a signed integer data type for information on 16-bit values using unsigned integers.)

## Digital I/O

Functions

UL: cbDIn(), cbDOut(), cbDBitIn(), cbDBitOut()

UL for .NET: DIn(), DOut(), DBitIn(), DBitOut()

PortNum

AUXPORT*

DataValue

0 to 255

BitNum

0 to 7

*AUXPORT is not configurable for these boards.

## Counter I/O

Functions

These boards do not have any counters and do not support any of the counter I/O functions.

## Hardware Considerations

##### Pacing analog input

Software pacing only