# CIO-DAS48-PGA, CIO-DAS48-I

The CIO-DAS48-PGA and CIO-DAS48-I supports the following UL and UL for .NET features.

## Analog Input

Functions

UL: cbAIn(), cbAInScan(), cbFileAInScan(), cbATrig()

UL for .NET: AIn(), AInScan(), FileAInScan(), ATrig()

Options

CONVERTDATA

HighChan

47 single-ended, 23 differential

Rate

Ignored

Range

The CIO-DAS48-PGA can be configured with a jumper for either voltage or current input. The CIO-DAS48-I is configured for current input only.

Voltage input ranges:

BIP10VOLTS (±10 volts) | UNI10VOLTS (0 to 10 volts)
BIP5VOLTS (±5 volts) | UNI5VOLTS (0 to 5 volts)
BIP2PT5VOLTS (±2.5 volt) | UNI2PT5VOLTS (0 to 2.5 volt)
BIP1PT25VOLTS (±1.25 volts) | UNI1PT25VOLTS (0 to 1.25 volts)
BIPPT625VOLTS (±0.625 volts) |

Current input ranges:

MA4TO20 (4 to 20 mA) | MA1TO5 (1 to 5 mA)
MA2TO10 (2 to 10 mA) | MAPT5TO2PT5 (0.5 to 2.5 mA)

## Notes

The CIO-DAS48/PGA and CIO-DAS48-I do not support analog output, digital I/O, or counter I/O functions.