List all options for specifying the counter mode.

class pyulwin.enums.CounterMode

Member | Value
BIT_16 | 0
BIT_32 | 4
BIT_48 | 65536
CLEAR_ON_READ | 1
COUNTER | 256
COUNT_DOWN_OFF | 0
COUNT_DOWN_ON | 65536
DECREMENT_OFF | 0
DECREMENT_ON | 32
ENCODER | 1280
ENCODER_MODE_BIT_32 | 4
ENCODER_MODE_BIT_48 | 65536
ENCODER_MODE_CLEAR_ON_Z_OFF | 0
ENCODER_MODE_CLEAR_ON_Z_ON | 32
ENCODER_MODE_LATCH_ON_Z | 8
ENCODER_MODE_MODULO_N_OFF | 0
ENCODER_MODE_MODULO_N_ON | 32768
ENCODER_MODE_NO_RECYCLE_OFF | 0
ENCODER_MODE_NO_RECYCLE_ON | 16384
ENCODER_MODE_RANGE_LIMIT_OFF | 0
ENCODER_MODE_RANGE_LIMIT_ON | 8192
ENCODER_MODE_X1 | 0
ENCODER_MODE_X2 | 1
ENCODER_MODE_X4 | 2
GATE_CLEARS_CTR | 524288
GATE_CONTROLS_DIR | 262144
GATE_TRIG_SRC | 1048576
GATING_OFF | 0
GATING_ON | 16
INVERT_GATE | 131072
LATCH_ON_MAP | 8
LATCH_ON_SOS | 0
MODULO_N_OFF | 0
MODULO_N_ON | 32768
NO_RECYCLE_OFF | 0
NO_RECYCLE_ON | 16384
OUTPUT_INITIAL_STATE_HIGH | 4194304
OUTPUT_INITIAL_STATE_LOW | 0
OUTPUT_ON | 2097152
PERIOD | 512
PERIOD_MODE_BIT_32 | 4
PERIOD_MODE_BIT_48 | 65536
PERIOD_MODE_GATING_ON | 16
PERIOD_MODE_INVERT_GATE | 131072
PERIOD_MODE_X1 | 0
PERIOD_MODE_X10 | 1
PERIOD_MODE_X100 | 2
PERIOD_MODE_X1000 | 3
PULSEWIDTH | 768
PULSEWIDTH_MODE_BIT_32 | 4
PULSEWIDTH_MODE_BIT_48 | 65536
PULSEWIDTH_MODE_GATING_ON | 16
PULSEWIDTH_MODE_INVERT_GATE | 131072
RANGE_LIMIT_OFF | 0
RANGE_LIMIT_ON | 8192
ROLLOVER | 0
STOP_AT_MAX | 2
TIMING | 1024
TIMING_MODE_BIT_32 | 4
TIMING_MODE_BIT_48 | 65536
TIMING_MODE_INVERT_GATE | 131072
TOTALIZE | 0
UPDOWN_OFF | 0
UPDOWN_ON | 4096