# CIO-DAS-TEMP

The CIO-DAS-TEMP supports the following UL and UL for .NET features.

## Temperature input

Functions

UL: cbTIn(), cbTInScan()

UL for .NET: TIn(), TInScan()

Options

NOFILTER

Scale

CELSIUS, FAHRENHEIT, KELVIN

HighChan

31

## Hardware considerations

##### Pacing Input

The rate of measurement is fixed at approximately 25 samples per second.

##### Selecting thermocouples

J, K, E, T, R, S or B type thermocouples may be selected using InstaCal.