List all options for specifying the analog input channel type.

class pyulwin.enums.AiChanType

Member | Value
CURRENT | 100
FULL_BRIDGE_62PT5mVV | 504
FULL_BRIDGE_7PT8mVV | 505
HALF_BRIDGE | 503
QUART_BRIDGE_120OHM | 502
QUART_BRIDGE_350OHM | 501
RESISTANCE_10K2W | 203
RESISTANCE_10K4W | 201
RESISTANCE_1K2W | 204
RESISTANCE_1K4W | 202
RTD_1000OHM_3W | 403
RTD_1000OHM_4W | 401
RTD_100OHM_3W | 404
RTD_100OHM_4W | 402
TC | 300
VOLTAGE | 0