# BoardConfig.GetAdTimingMode() method

Returns the ADC timing mode.

Member of the cBoardConfig class. Accessible from the MccBoard.BoardConfig property.

## Function Prototype

VB .NET

Public Function GetAdTimingMode(ByRef configVal As Integer) As MccDaq.ErrorInfo

C# .NET

public MccDaq.ErrorInfo GetAdTimingMode(out int configVal)

## Parameters

configVal

Returns the ADC timing mode – 1 (High Speed), 8 (60 Hz rejection), 9 (50 Hz rejection), or 15 (High resolution).

## Returns

- An ErrorInfo object that indicates the status of the operation.