# PCI-DAC6702, PCI-DAC6703

The PCI-DAC6702 and PCI-DAC6703 support the following UL and UL for .NET features.

## Analog output

Functions

UL: cbAOut(), cbVOut(), cbAOutScan()

UL for .NET: AOut(), VOut(), AOutScan()

HighChan

PCI-DAC6702: 7

PCI-DAC6703: 15

Count

HighChan - LowChan + 1 max

Rate

Ignored

Range

Ignored - Not programmable; fixed at BIP10VOLTS (± 10.1 V)

DataValue

0 to 65,535 (Refer to 16-bit values using a signed integer data type for information on 16-bit values using unsigned integers.)

## Digital I/O

Functions

UL: cbDOut(), cbDIn(), cbDBitIn(), cbDBitOut(), cbDConfigPort(), cbDConfigBit()

UL for .NET: DOut(), DIn(), DBitIn(), DBitOut(), DConfigPort(), DConfigBit()

PortNum

AUXPORT is bitwise configurable for these boards, and must be configured using cbDConfigBit() or cbDConfigPort() before use as output.

DataValue

0 to 255

BitNum

0 to 7

## Configuration

Functions

UL: cbGetConfig(), cbSetConfig()

UL for .NET: GetDACStartup(), GetDACUpdateMode(), SetDACStartup(), SetDACUpdateMode()

ConfigItem

BIDACSTARTUP, BIDACUPDATEMODE, BIDACUPDATECMD

## Hardware considerations

##### Pacing analog output

Software only