# CIO-DAS800 Series

The CIO-DAS800 Series includes the following hardware:

- CIO-DAS800
- CIO-DAS801
- CIO-DAS802
- CIO-DAS802/16

CIO-DAS800 Series supports the following UL and UL for .NET features.

## Analog Input

Functions

UL: cbAIn(), cbAInScan(), cbATrig(), cbFileAInScan()

UL for .NET: AIn(), AInScan(), ATrig(), FileAInScan()

Options

BACKGROUND, CONTINUOUS, EXTCLOCK, CONVERTDATA, SINGLEIO, BLOCKIO, EXTTRIGGER

HighChan

0 to 7

Rate

CIO-DAS802/16:

100,000

All others in the series:

50,000

Range

CIO-DAS800:

Ignored - Not programmable

CIO-DAS801:

BIP10VOLTS (±10 volts) | UNI10VOLTS (0 to 10 volts)
BIP5VOLTS (±5 volts) | UNI1VOLTS (0 to 1 volts)
BIP1VOLTS (±1 volts) | UNIPT1VOLTS (0 to 0.1 volts)
BIPPT5VOLTS (±0.5 volts) | UNIPT01VOLTS (0 to 0.01 volts)
BIPPT05VOLTS (±0.05 volts) |
BIPPT01VOLTS (±0.01 volts) |

CIO-DAS802:

BIP10VOLTS (±10 volts) | UNI10VOLTS (0 to 10 volts)
BIP5VOLTS (±5 volts) | UNI5VOLTS (0 to 5 volts)
BIP2PT5VOLTS (±2.5 volts) | UNI2PT5VOLTS (0 to 2.5 volts)
BIP1PT25VOLTS (±1.25 volts) | UNI1PT25VOLTS (0 to 1.25 volts)
BIPPT625VOLTS (±0.625 volts) |

CIO-DAS802/16:

BIP10VOLTS (±10 volts) | UNI10VOLTS (0 to 10 volts)
BIP5VOLTS (±5 volts) | UNI5VOLTS (0 to 5 volts)
BIP2PT5VOLTS (±2.5 volts) | UNI2PT5VOLTS (0 to 2.5 volts)
BIP1PT25VOLTS (±1.25 volts) | UNI1PT25VOLTS (0 to 1.25 volts)

## Analog output

These boards do not have D/A converters, and do not support analog output functions.

## Digital I/O

Functions

UL: cbDIn(), cbDOut(), cbDBitIn(), cbDBitOut()

UL for .NET: DIn(), DOut(), DBitIn(), DBitOut()

PortNum

AUXPORT (not configurable for these boards)

DataValue

UL: 0 to 15 using cbDOut(), 0 to 7 using cbDIn()

UL for .NET: 0 to 15 using DOut(), 0 to 7 using DIn()

BitNum

0 to 3 using cbDBitOut()/DBitOut()

0 to 2 using cbDBitIn()/DBitIn()

## Counter I/O

Functions

UL: cbC8254Config(), cbCIn(), cbCLoad()

UL for .NET: C8254Config(), CIn(), CLoad()

CounterNum

1 to 3

Config

HIGHONLASTCOUNT, ONESHOT, RATEGENERATOR, SQUAREWAVE, SOFTWARESTROBE, HARDWARESTROBE

LoadValue

0 to 65,535 (Refer to 16-bit values using a signed integer data type for information on 16-bit values using unsigned integers.)

## Hardware considerations

##### Pacing analog input

Hardware pacing, external or internal clock supported.

The packet size is 128 samples.

Note that digital output is not compatible with concurrent cbAInScan()/AInScan() operation, since the channel multiplexor control shares the register with the digital output control. Writing to this register during a scan may adversely affect the scan.

##### Triggering and gating

Digital hardware triggering supported.