# Supported A/D Ranges for UL

The table below lists the constants you can use in the Range argument and the cbALoadQueue() method's gainArray parameter. Valid ranges for your hardware are listed in the Universal Library User’s Guide.

Constant name | Range | Value
BIP60VOLTS | ±60 volts | 20
BIP20VOLTS | ±20 volts | 15
BIP15VOLTS | ±15 volts | 21
BIP10VOLTS | ±10 volts | 1
BIP5VOLTS | ±5 volts | 0
BIP4VOLTS | ±4 volts | 16
BIP2Pt5VOLTS | ±2.5 volts | 2
BIP2VOLTS | ±2 volts | 14
BIP1Pt67VOLTS | ±1.67 volts | 11
BIP1Pt25VOLTS | ±1.25 volts | 3
BIP1VOLTS | ±1 volts | 4
BIPPT625VOLTS | ±0.625 volts | 5
BIPPT5VOLTS | ±0.5 volts | 6
BIPPT312VOLTS | ±0.3125 volts | 17
BIPPT25VOLTS | ±0.25 volts | 12
BIPPT2VOLTS | ±0.2 volts | 13
BIPPT156VOLTS | ±0.15625 volts | 18
BIPPT125VOLTS | ±0.125 volts | 22
BIPPT1VOLTS | ±0.1 volts | 7
BIPPT078VOLTS | ±0.078125 volts | 19
BIPPT05VOLTS | ±0.05 volts | 8
BIPPT01VOLTS | ±0.01 volts | 9
BIPPT005VOLTS | ±0.005 volts | 10
UNI10VOLTS | 0 - 10 volts | 100
UNI5VOLTS | 0 - 5 volts | 101
UNI4VOLTS | 0 - 4 volts | 114
UNI2Pt5VOLTS | 0 - 2.5 volts | 102
UNI2VOLTS | 0 - 2 volts | 103
UNI1Pt67VOLTS | 0 - 1.67 volts | 109
UNI1Pt25VOLTS | 0 - 1.25 volts | 104
UNI1VOLTS | 0 - 1 volts | 105
UNIPt5VOLTS | 0 - 0.5 volts | 110
UNIPt25VOLTS | 0 - 0.25 volts | 111
UNIPt2VOLTS | 0 - 0.2 volts | 112
UNIPt1VOLTS | 0 - 0.1 volts | 106
UNIPt01VOLTS | 0 - 0.01 volts | 107
UNIPt02VOLTS | 0 - 0.02 volts | 108
UNIPt05VOLTS | 0 - 0.05 volts | 113
MA4TO20 | 4 - 20 mA | 200
MA2TO10 | 2 - 10 mA | 201
MA1TO5 | 1 - 5 mA | 202
MAPt5TO2pt5 | 0.5 - 2.5 mA | 203
MA0TO20 | 0 - 20 mA | 204
BIPPT025AMPS | ±0.025 amps | 205
Not Used |  | –1