# d_out_array()

Sets the values of specified ports simultaneously.

## Prototype

d_out_array(board_num, low_port, high_port, data_list)

## Parameters

board_num (int)

The number associated with the board when it was installed with InstaCal or created with create_daq_device().

low_port (DigitalPortType)

The first port in the scan.

high_port (DigitalPortType)

The last port in the scan.

data_list (list of int)

Digital output data list.