# BoardConfig.GetDACStartup() method

Returns the board's configuration register STARTUP bit setting. Refer to SetDACStartup() Notes section for more information.

Member of the cBoardConfig class. Accessible from the MccBoard.BoardConfig property.

## Function Prototype

VB .NET

Public Function GetDACStartup(ByVal devNum As Integer, ByRef configVal As Integer) As MccDaq.ErrorInfo

C# .NET

public MccDaq.ErrorInfo GetDACStartup(int devNum, out int configVal)

## Parameters

devNum

The number of the DAC channel whose startup bit setting you want to get.

configVal

The setting of the startup bit (0 or 1).

## Returns

- An ErrorInfo object that indicates the status of the operation.
- configVal - Returns 0 if the startup bit is disabled, or 1 if the startup bit is enabled.