# BoardConfig.SetExpDetectOpenTc()

Sets the open thermocouple detection state of an expansion board.

Member of the cBoardConfig class. Accessible from the MccBoard.BoardConfig property.

## Function Prototype

VB .NET

Public Function SetExpDetectOpenTc(channel As Integer, enable As Integer) As MccDaq.ErrorInfo

Public Function SetExpDetectOpenTc(enable As Integer) As MccDaq.ErrorInfo

C# .NET

public MccDaq.ErrorInfo SetExpDetectOpenTc(int channel, int enable)

public MccDaq.ErrorInfo SetExpDetectOpenTc(int enable)

## Parameters

channel

The temperature input channel number.

enable

The open thermocouple detection setting. 0 = disable; 1 = enable.

## Returns

- An ErrorInfo object that indicates the status of the operation.