# PPIO-AI08

The PPIO-AI08 supports the following UL and UL for .NET features.

## Analog Input

Functions

UL: cbAIn(), cbAInScan(), cbATrig(), cbFileAInScan()

UL for .NET: AIn(), AInScan(), ATrig(), FileAInScan()

Options

CONVERTDATA

HighChan

0 to 7

Rate

Ignored

Range

This board does not have programmable gain, so the Range argument to analog input functions is ignored.

## Digital I/O

Functions

UL: cbDIn(), cbDOut(), cbDBitIn(), cbDBitOut()

UL for .NET: DIn(), DOut(), DBitIn(), DBitOut()

PortNum

AUXPORT*

DataValue

0 to 15 using cbDOut() or DOut()

0 to 7 using cbDIn() or DIn()

BitNum

0 to 3 using cbDBitOut() or DBitOut()

0 to 2 using cbDBitIn() or DBitIn()

* AUXPORT is not configurable for this board.

## Hardware Considerations

##### Pacing analog input

Software pacing only