# BoardConfig.GetSyncMode()

Returns the simultaneous mode setting of supported analog output devices.

Member of the cBoardConfig class. Accessible from the MccBoard.BoardConfig property.

## Function Prototype

VB .NET

Public Function GetSyncMode(ByRef configVal As Integer) As MccDaq.ErrorInfo

C# .NET

public MccDaq.ErrorInfo GetSyncMode(out int configVal)

## Parameters

configVal

Returns the simultaneous mode setting – 0 (Master mode), or 1 (Slave mode).

## Returns

- An ErrorInfo object that indicates the status of the operation.