# DaqDeviceManager class

Contains all of the members for discovering USB, Bluetooth, and Ethernet devices without using InstaCal.

The DaqDeviceManager class is a member of the MccDaq namespace. Refer to the Universal Library Language Interface for an explanation of the MccDaq namespace.

## Methods

The DaqDeviceManager class contains the following methods:.

- GetDaqDeviceInventory() – Detects USB, Bluetooth, and Ethernet DAQ devices, and returns device desciptors of the detected devices.
- CreateDaqDevice() – Creates a device object for the specified DAQ device within the Universal Library, and assigns the specified board number to the DAQ device.
- ReleaseDaqDevice() – Removes the specified DAQ device from the UL and releases all resources associated with that device.
- GetNetDeviceDescriptor() – Returns the DAQ device descriptor at the specified IP address or host name.
- GetBoardNumber() – Returns information about a DAQ device.
- IgnoreInstaCal() – Prevents the Universal Library from automatically adding a DAQ device that has been stored in the cb.cfg file by InstaCal.