# BoardConfig.SetPatternTrigPort()

Sets the pattern trigger port.

Member of the cBoardConfig class. Accessible from the MccBoard.BoardConfig property.

## Function Prototype

VB .NET

Public Function SetPatternTrigPort(ByRef configVal As Integer) As MccDaq.ErrorInfo

C# .NET

public MccDaq.ErrorInfo SetPatternTrigPort(int configVal)

## Parameters

configVal

Sets the pattern trigger port (1= AuxPort or AuxPort0, 2 = AuxPort1).

## Returns

- An ErrorInfo object that indicates the status of the operation.